**RA1911029010074**

**SREELAKSHMI NAMBIAR**

**AIM**- Setting Password to a router

**PROCEDURE**

Enter no to enter into the user execution mode which shows router>

Then enter enable this has allowed us to enter into the privilleged execution mode which is router#

Not enter config t it will show router(config)#

Interface fastethernet 0/0

Ip address 10.0.0.1 255.0.0.0

No shutdown

Exit this exists from config if to config

Line vty 0 4

Password cisco

Login

Exit

Line console 0

Password cisco

Login

Exit

Enable secret cisco -by this process the password is encrypted

**RESULT**

Password is set for the router is set

**<images attached below>**





